IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-11-22T23:18:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170118_1100(x64) - Exporter 17.0.1117.0 - Alternate UI 19.1.0.0"
Application: "Autodesk Revit 2017 (RUS)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (RUS)"

People and organizations
  Person "TAlex" of Organization (no name given)
  Owner history of Person "TAlex" of Organization (no name given) | application "Autodesk Revit 2017 (RUS)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (RUS)" | change NOCHANGE | created 1606075115 (2020-11-22T19:58:35Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 55° 44′ 59.999999″ | longitude 37° 42′ 0.002746″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Москва", "Россия"
      IFCBUILDINGSTOREY "Этаж 01" | long name "Этаж 01" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Конвектор_Шириной 250мм_6трубный" | object type "Конвектор_Шириной 250мм_6трубный" | names: "BIMLIB_Конвектор_НапольныйСЕстественнойКонвекцией_ВКН400_VITRON:Конвектор_Шириной 250мм_6трубный:1278422" | material: materials ("BIMLIB_Алюминий_VITRON", "BIMLIB_УГО1_VITRON", "BIMLIB_ОцинкованнаяСталь_VITRON") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_SpaceHeaterTypeCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Конвектор_Шириной 250мм_6трубный" | 1 occurrence | material: materials ("BIMLIB_Алюминий_VITRON", "BIMLIB_УГО1_VITRON", "BIMLIB_ОцинкованнаяСталь_VITRON")

Property sets
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Конвектор_Шириной 250мм_6трубный" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Вилма / VITRON" (IFCLABEL)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    ADSK_URL документации изделия = "https://vitron.ru/katalog-konvektor-prise#vysota-400-mm" (IFCTEXT)
    ADSK_URL страницы изделия = "https://vitron.ru/vkn-400-mm/konvektory-vodyanye-napolnye-vkn-400-250-6tp" (IFCTEXT)
    ADSK_Единица измерения = "шт." (IFCTEXT)
    ADSK_Код изделия = "ВКН.400.250.1000.6ТП" (IFCTEXT)
    ADSK_Код изделия = "ВКН.400.250.1000.6ТП" (IFCTEXT)
    ADSK_Марка = "ВКН.400.250.1000.6ТП" (IFCTEXT)
    ADSK_Масса = 17.464322970833 (IFCREAL)
    ADSK_Наименование = "Конвектор напольный с естественной конвекцией ВКН.400.250.1000.6ТП" (IFCTEXT)
    ADSK_Обозначение = "ВКН.400.250" (IFCTEXT)
    ADSK_Потеря давления жидкости = 946.724286736749 (IFCREAL)
    ADSK_Размер_Высота = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    ADSK_Размер_Диаметр = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    ADSK_Размер_Длина = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ADSK_Размер_Ширина = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    ADSK_Расход жидкости = 1.07639104167097 (IFCLENGTHMEASURE) [MILLI METRE]
    ADSK_Тепловая мощность = 33310.0187033707 (IFCREAL)
    BL_BIM library = "https://bimlib.pro/manufacturer/company/21564" (IFCTEXT)
    BL_Email = "info@vitron.ru" (IFCTEXT)
    BL_Разработано = "support@bimlib.ru" (IFCTEXT)
    URL = "https://vitron.ru" (IFCTEXT)
    VIT_Максимальная рабочая температура теплоносителя = 368.15 (IFCREAL)
    VIT_Рабочее давление теплоносителя = 487680. (IFCREAL)
    VIT_Тепловая мощность на 1 м = 33310.0187033707 (IFCREAL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)